In this section you will identify electromagnetic (EM) spectrum and electromagnetic environmental effects (E3) control requirements and ensure compliance with appropriate policy and guidance. This information supports compliance with System Survivability KPP and Force Protection KPP.

- The spectrum supportability process includes joint, DoD, national and international policies and procedures for the management and use of the EM spectrum.

- The spectrum supportability process is detailed in Annex A to Appendix G to Enclosure B, JCIDS Manual. Details on compliance are available in:

- DoDI 8320.05, Electromagnetic Spectrum Data Sharing

- DoDI 4650.01, Policy and Procedures for Management and Use of the Electromagnetic Spectrum.

- Note: The Content Guide for the Net-Ready KPP Wiki (referred to in Section 7) is listed as a reference for this section in the JCIDS Manual; however, while it contains a lot of material on net-ready it does not seem to cover Spectrum and E3 Control.

- IAW DoDI 4650.01, spectrum certification, Host Nation coordination/ approval, and spectrum supportability risk assessment (SSRA) requirements should be addressed/summarized in this paragraph.

- All electrical and electronic systems, subsystems, and equipment, including ordnance, must comply with E3 direction IAW DoDI 8500.01, Cybersecurity.

- State the intent to design these systems to JTSE standards and discuss technical approaches to ensure technical interoperability.

- JTSE standards are maintained in the DoD IT Standards Registry (DISR) (CAC required),

- Other applicable spectrum related requirements that may be included:

- Bandwidth, quality of service, and spectrum data capture requirements for DoD by DoD and Federal spectrum certification as described in DoDI 4650.01.

- If the capability will interface with the Joint Worldwide Intelligence Communications System (JWICS) or other intelligence-managed dissemination systems to receive or transmit information, bandwidth requirements and quality of service requirements must be addressed.

- Ensure consistency with any identified intelligence interoperability requirements consistent with Annex G to Appendix G of Enclosure B, JCIDS Manual.

- If there are potential issues regarding E3 interference from threat emitters, ensure these issues are identified in this section.

- Ensure this section is consistent with the threat discussion in Section 2 and in the threat products from DIE including, but not limited to, the Validated On-line Life-cycle Threat (VOLT) report (contact your PMO team members for a copy of the VOLT).