2.5.1.5. Section 5: Performance Attributes (KPPs, KSAs, and APAs). Follows the same format as a regular CDD with the exception of the following:

2.5.1.5.1. Performance attributes may be quantified in terms of initial minimum values rather than threshold/objective values. As with regular CDDs, the performance attributes must reflect performance that satisfies the CRs identified in Section 3 of the IS-CDD. Reference Figure B-13, under paragraph 2.5.7.1, of this manual as an example of how to capture the Net- Ready performance attributes for an IS-CDD.

2.5.1.5.2. Mandatory KPPs/Attributes. The mandatory KPP/Attributes apply to an IS-CDD. The SS KPP and Sustainment KPP are required for the IS-CDD. The Interoperability Attribute, Joint or otherwise will also be addressed along with Exportability.

2.5.1.5.2.1. SS KPP. For an IS-CDD, the SS should focus on the ability of the system to operate in a cyber and EMS-contested environment as per Annex C to Appendix G of this enclosure. The following shall be included under the SS KPP:

2.5.1.5.2.1.1. Identify the CSRC, EMS Survivability Risk Category, and how they were determined (for Cyber, specify if it was determined using the CSEIG- recommended approach);

2.5.1.5.2.1.2. Include tailored language for the CDD (tailored for an IS-CDD);

2.5.1.5.2.1.3. Address the Cyber Survivability Pillars (Prevent, Mitigate, and Recover from Cyber Events) and the associated Cyber Survivability Attributes (CSAs) (1-10), as applicable. This information can be provided in a table or, as needed, in the associated narrative. For more information, see the CSE Implementation Guide, via KM/DS additional guidance.

2.5.1.5.2.1.4. For EMS Survivability, see Annex C to Appendix G of this enclosure and the EMS Survivability Guidebook, via KM/DS (Reference [4]).

2.5.1.5.2.2. Sustainment KPP. For an IS-CDD the Sponsor should focus the Sustainment KPP on the operational availability of the IS solution as per Annex D to Appendix G of this enclosure.

For reference or comparison, below is what the JCIDS Manual says for the CDD 2021 itself:

2.5.5.3. Present each performance attribute (KPP, KSA, or APA) in terms of parameters needed to address the validated requirements consistent with the DoDAF CV-3.

2.5.5.3.1. The performance attributes reflect Measures of Performance (MOPs) for the system being developed and not Measures of Effectiveness (MOEs) in conducting the mission. Ensure parameters chosen are technically achievable, quantifiable, measurable, testable, unambiguous, supported by documented trade-off analysis, and defined in a manner that supports efficient and effective T&E.

2.5.5.3.2. Provide threshold values for each performance attribute that represent the value below which performance would require reevaluation of military utility in the applicable CONOPS and/or Operational Mode Summary/Mission Profile (OMS/MP). Provide objective values in cases where the increased performance level of a parameter provides significant increases in operational utility.

2.5.5.3.3. Provide a range between threshold and objective values to allow trade space to explore during the TMRR and EMD phase of acquisition without having to revalidate the CDD to pursue different levels of performance. The PM may use this information to provide incentives for the development contractor or to weigh capability tradeoffs between threshold and objective values. Trade space should be sufficient to allow for increased capability in the future due to evolving technology, threat, or interoperability needs.

2.5.5.4. Address the mandatory attributes Energy KPP, SS KPP, Force Protection KPP, and Sustainment KPP, Interoperability JPR/KPP/KSA andExportability KSA and provide all applicable Tables.

2.5.5.5. The Interoperability performance attribute (JPR, KPP, KSA) is required to be addressed by the Sponsor in Section 5 Tables as depicted in Figures B-8through B-10 along with attributes for Net-Ready, Physical Interoperability, and Joint Training Technical Interoperability (JTTI) (KPP, KSA, APA) if applicable.

2.5.5.5.1. For Net-Ready, include the Performance Attribute Table that presents the Net-Ready performance attributes and their associated metrics in terms of a standardized framework and data sources to leverage when developing attributes and their threshold and objective values. The Net-Ready Attribute Table includes: Support of Military Operations, Entered and be Managed on the Network, and Exchange Information as depicted in Figure B- 11.