2.5.1.6. Section 6: Other System Attributes. Optional for an IS-CDD with the exception of consideration should be given to identify the system categorization for information systems as a required capability - the potential impact (low, moderate, or high) resulting from loss of confidentiality, integrity, and availability, if a security breach occurs IAW Reference [36].

For reference or comparison, below is what the JCIDS Manual says for the DCR 2025 itself:

2.5.6. Other System Attributes.

2.5.6.1. The purpose of this Section is to identify any other system attributes not directly quantified (as performance attributes) and traceable to operational performance, and not identified elsewhere in the document.

2.5.6.2. Other system attributes may include the following:

2.5.6.2.1. Future integration platforms. Used in cases where integration on certain platforms is not currently planned or resourced, not already captured in the IOC and FOC definitions in the Program Summary Section of the ICD (Section 4), but the Sponsor would like to preserve the option for future integration on additional platforms.

2.5.6.2.2. Embedded instrumentation, electromagnetic attack, and wartime reserve mode (WARM) requirements.

2.5.6.2.3. Human Systems Integration (HSI) considerations that have a major impact on system effectiveness, suitability, and survivability. The HSI Force Protection and Survivability domain contributes to the Force Protection KPP by defining requirements for personnel force protection and personnel survivability. The HSI Safety and Occupational Health domain contributes to the Force Protection KPP by defining requirements for personnel and system safety. DOTmLPF-P analyses should identify and address HSI.

2.5.6.2.4. Environmental design to the specific environmental/climatic conditions an equipment item is likely to encounter during its service life to include natural environmental factors, including climatic design type, terrain, meteorological and oceanographic (METOC) factors, impacts, and effects.

2.5.6.2.5. Weather, oceanographic and astro-geophysical support needs throughout the program�s projected lifecycle, including data accuracy and forecast needs.

2.5.6.2.6. Transportability and deployability considerations, IAW Reference [41], will include how the capability solution and related materiel will be moved either to or within the theater, and identify any lift limitations.

2.5.6.2.7. Space, Weight, & Power, and Cooling (SWAP-C) margin requirements and open system attributes, to ensure future flexibility and upgradability of systems and sub-systems to changing technologies and threats.

2.5.6.2.8. Derived system requirements to support systems that may be used in allied, partner-nation, coalition, or multinational operations relating to U.S.-ratified international standardization agreements, IAW References [41], [42], [43], and [44].

2.5.6.2.9. Cybersecurity Risk Management for DoD Systems: In addition, the IS-CDD must identify the system categorization for systems as a required capability - the potential impact (low, moderate, or high) resulting from loss of confidentiality, integrity, and availability if a security breach occurs.