2.5.1.5. Section 5: Performance Attributes (KPPs, KSAs, and APAs). Follows the same format as a regular CDD with the exception of the following:

2.5.1.5.1. Performance attributes may be quantified in terms of initial minimum values rather than threshold/objective values. As with regular CDDs, the performance attributes must reflect performance that satisfies the CRs identified in Section 3 of the IS-CDD. Reference Figure B-13, under paragraph 2.5.7.1, of this manual as an example of how to capture the Net- Ready performance attributes for an IS-CDD.

2.5.1.5.2. Mandatory KPPs/Attributes. The mandatory KPP/Attributes apply to an IS-CDD. The SS KPP and Sustainment KPP are required for the IS-CDD. The Interoperability Attribute, Joint or otherwise will also be addressed along with Exportability.

2.5.1.5.2.1. SS KPP. For an IS-CDD, the SS should focus on the ability of the system to operate in a cyber and EMS-contested environment as per Annex C to Appendix G of this enclosure. The following shall be included under the SS KPP:

2.5.1.5.2.1.1. Identify the CSRC, EMS Survivability Risk Category, and how they were determined (for Cyber, specify if it was determined using the CSEIG- recommended approach);

2.5.1.5.2.1.2. Include tailored language for the CDD (tailored for an IS-CDD);

2.5.1.5.2.1.3. Address the Cyber Survivability Pillars (Prevent, Mitigate, and Recover from Cyber Events) and the associated Cyber Survivability Attributes (CSAs) (1-10), as applicable. This information can be provided in a table or, as needed, in the associated narrative. For more information, see the CSE Implementation Guide, via KM/DS additional guidance.

2.5.1.5.2.1.4. For EMS Survivability, see Annex C to Appendix G of this enclosure and the EMS Survivability Guidebook, via KM/DS (Reference [4]).

2.5.1.5.2.2. Sustainment KPP. For an IS-CDD the Sponsor should focus the Sustainment KPP on the operational availability of the IS solution as per Annex D to Appendix G of this enclosure.

For reference or comparison, below is what the JCIDS Manual says for the CDD 2021 itself:

2.5.5.2.4. If the CDD is describing a FoS solution as the base CDD, it must describe the overall performance attributes for the FoS level of performance. Any unique performance attributes for each of the constituent systems will be documented in separate CDD Annexes.